{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet 1","index":0,"n_rows":3,"n_cols":11,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["MATERIAL CODE","DESCRIPTION","NOUN","MODIFIER","TASK INCLUDE","TYPE","SIZE","MATERIAL","RATING","ADDITIONAL DETAILS","LONG DESC"]
["LF3699540116","PROVIDING AND FIXING FIXED/SIDE HUNG OPENABLE WINDOWS AS PER THE DWGS FROM OF HEAVY DUTY AL EXTRUDED PROFILES POLYURETHANE POLYESTER POWDER COATED 60-65MICRONS DFT,AS PER APPROVED COLOR AND SHADE SIZE:W10 4000 X 1450MM","SUPPLY AND FIXING","CIVIL",null,"FIXED/SIDE HUNG OPENABLE WINDOWS","SHADE SIZE:W10 4000 X 1450  MM",null,null,"AS PER THE DWGS FROM OF HEAVY DUTY AL EXTRUDED PROFILES POLYURETHANE POLYESTER POWDER COATED 60-65 MICRONS DFT,AS PER APPROVED COLOR","SUPPLY AND FIXING,CIVIL,TYPE:FIXED/SIDE HUNG OPENABLE WINDOWS,SIZE:SHADE SIZE:W10 4000 X 1450  MM,ADDITIONAL DETAILS:AS PER THE DWGS FROM OF HEAVY DUTY AL EXTRUDED PROFILES POLYURETHANE POLYESTER POWDER COATED 60-65 MICRONS DFT,AS PER APPROVED COLOR"]
["LF3699540099","PROVIDING AND FIXING FIXED/SIDE HUNG OPENABLE WINDOWS AS PER THE DWGS FROM OF HEAVY DUTY AL EXTRUDED PROFILES POLYURETHANE POLYSTER POWDER COATED 60-65MICRONS DFT,AS PER APPROVED COLOR AND SHADE,SIZE:V1 600 X 600MM","SUPPLY AND FIXING","CIVIL",null,"FIXED/SIDE HUNG OPENABLE WINDOWS","SHADE SIZE:V1 600 X 600 MM",null,null,"AS PER THE DWGS FROM OF HEAVY DUTY AL EXTRUDED PROFILES POLYURETHANE POLYESTER POWDER COATED 60-65 MICRONS DFT,AS PER APPROVED COLOR","SUPPLY AND FIXING,CIVIL,TYPE:FIXED/SIDE HUNG OPENABLE WINDOWS,SIZE:SHADE SIZE:V1 600 X 600 MM,ADDITIONAL DETAILS:AS PER THE DWGS FROM OF HEAVY DUTY AL EXTRUDED PROFILES POLYURETHANE POLYESTER POWDER COATED 60-65 MICRONS DFT,AS PER APPROVED COLOR"]